**Unverferth Talc & Graphite Flow Kit to update T&G Applicator**

This update kit from Unverferth has been demonstrated as a viable application solution for Low Mu Tech Dust. Please contact your location Unverferth or Brent dealer to order a kit for use with your respective applicator/tender models.

**The full kit and parts breakdown are as follows:**

**Full Kit: (order this full kit to replace the current items listed below)**

T & G Flow Kit: 2003214 – $210 suggested retail (56 inch Auger, PVC pipe, Flow Screen, Coupler with hose clamps)

**Individual Parts: ( Order any individual parts here as may be needed or indicated if not ordering full kit initially or for repair/replacement parts)**

Flow Screen: 33083 - $48 suggested retail

Rubber Coupler with hose clamps: 9500585 - $9 suggested retail

Black PVC spout: 2003217 - $90 suggested retail

56 inch Auger flighting: 2003215 - $83 suggested retail

* This will work for any current production Unverferth seed-tender with side mount T & G applicator.
* If you or your customer has older style unit that is a rear mount, these are ones with 70” plus spouts, we would not have a longer auger than what is already in the system.
  + Customer could order the coupler and screen. if this would suffice these would be Unverferth item numbers 33083 for the screen, and 9500585 for the coupler with hose clamps.

Estimated Installation time: 1 to 2 hours – Use Unverferth installation instructions.

